*******************************************************************************
   Jz4740 USB tools

  Made by Maurus Cuelenaere for Rockbox
  Copyright (C) 2008
*******************************************************************************

To compile usbtools, you'll need jz_xloader (which can be get at
http://repo.or.cz/w/jz_xloader.git, do
"git clone git://repo.or.cz/jz_xloader.git ." for a clone in the current dir).

When you're on Linux, just type "make linux" to compile all the utilities (make
sure you have libusb-dev installed).
For cleaning: "make clean-linux"

When you're on Windows, install MingW32 and LibUSB-Win32 and edit "Makefile" to
make sure "WIN_DRIVERS_LIBUSB_DIR" is set correctly.
For cleaning: "make clean-win"

When Windows pops up the window when it needs drivers for a "Jz4740 USB Boot
Device" (VID=601A, PID=4740), point it to the windows_driver/ directory.

On Linux there's no driver installation, everything is handled through LibUSB.

That's all!

More info/tools:
  * http://www.rockbox.org/wiki/ChinaChip

 ***************************************************************************
 *             __________               __   ___.
 *   Open      \______   \ ____   ____ |  | _\_ |__   _______  ___
 *   Source     |       _//  _ \_/ ___\|  |/ /| __ \ /  _ \  \/  /
 *   Jukebox    |    |   (  <_> )  \___|    < | \_\ (  <_> > <  <
 *   Firmware   |____|_  /\____/ \___  >__|_ \|___  /\____/__/\_ \
 *                     \/            \/     \/    \/            \/
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License
 * as published by the Free Software Foundation; either version 2
 * of the License, or (at your option) any later version.
 *
 * This software is distributed on an "AS IS" basis, WITHOUT WARRANTY OF ANY
 * KIND, either express or implied.
 *
 ****************************************************************************
